WIN

OUT

DOWNWARD MOVEMENT

UPWARD MOVEMENT

IR SENSOR

OBSTACLES MOVEMENT

CAR -ARDUINO NANO

RECEIVE SIGNAL FROM BLUETOOTH MODULE

INPUT ‘X’

X==0 X==1

GREEN

RED